**USCG Local Notice to Mariners:**

**Allegheny River, Mile 28.6 – BRIDGE CONSTRUCTION**

**Freeport Bridge**; the land based approaching spans on the LDB are being demolished and rebuilt. The later phase of the rehab will require steel repairs and re-decking work on the channel span and a containment platform may extend 5 feet below low steel for a reduced clearance of 42 feet above normal pool. The project is scheduled to be completed November 28, 2013.

**Allegheny River, Mile 21.8 – BRIDGE CONSTRUCTION**

**Tarentum Highway Bridge**; deck repairs and spot painting are in progress until October 31, 2013, Monday through Friday, during daylight hours. The work will not interfere with waterway navigation. For additional information mariners may call (724) 323-5317.

**Monongahela River, Mile 127.4 – BRIDGE MAINTENANCE**

**Third Street Bridge (David Morgan Memorial Bridge);** a containment system is extending 5 feet below low steel while maintenance is being conducted on the subject bridge. Work will be performed 7-days a week, from 7:00 a.m. until 7:00 p.m., until August 31, 2013. For additional information mariners may contact the site supervisor by cell phone at (727) 460-6511 or (727) 460-8074.

**Monongahela River, Mile 41.0-BRIDGE INFORMATION**

**Charleroi-Monessen Bridge**; Due to shoaling approximately 140 feet channel ward from the left descending pier, the red channel margin lights located both upstream and downstream on the left descending side have been moved to mark the edge of this shoaling. Both center green range navigation lights have also been moved approximately 70 feet channel ward to indicate the center of the navigation channel. The horizontal clearance has been reduced to 335 feet.

**Monongahela River, Mile 16.6 - BRIDGE MAINTENANCE**

**William D. Mansfield Memorial Bridge**; due to a containment system, the vertical clearance in the channel span has been reduced to 62.3 feet above pool stage. Work will be conducted from 7:00 a.m. until 5:00 pm., Monday through Saturday. Mariners are urged to transit the bridge with caution.

**Ohio River, Mile 16.8 – BRIDGE MAINTENANCE**

**Ambridge-Aliquippa Bridge**; The vertical clearance is reduced by 3 feet due to a containment extending below the low steel. Also equipment may extend 12 feet into the channel for pier repair work. Work will be conducted during daylight hours, Monday through Friday, until October 2013. Contact the Trumbull Corp. at (724) 333-6542 or (412) 292-9642, for status.

**USCG Safety Zone/Marine Events:**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **WATERWAY** | **DATE** | **TIME** | **EVENT NAME** | **TYPE OF EVENT** | **SAFETY ZONE/ SAFETY ADVISORY/ LNM** | **River Closure** |
| Allegheny River, Mile 00.3 - 000.7 | 08/31/2013 | 2000 to 2300 | Pittsburgh Pirates Sky Blast | Barge Based Fireworks Display | Safety Zone/LNM | Full River |
| Ohio River, Mile 090.4 -90.8 | 08/31/2013 to  09/01/2013 | 0900 to 1800 | Wheeling Vintage Raceboat Regatta | Regatta | Safety Zone/LNM | Full River |
| Monongahela River, Mile .22-.77 | 09/17/2013 | 2030 to 2145 | Riverhounds Post Game Fireworks Display | Barge Based Fireworks | Safety Zone/LNM | Full |
| Ohio River, Mile 1.5 - Allegheny River, Mile 0.6 | 09/23/2013 | 1800 to 2100 | Pittsburgh International Festival of Firsts - Florentijn Hofman Duck | Art Exhibit | Safety Advisory | No |